2.5.5 Configure Initial Switch Settings

Part 1:

Step 2:

- 24 Fast Ethernet Interfaces

* 2 Gigabit Ethernet Interfaces
* The range of values shown for the vty lines is from 0 to 15
* show startup-config
* Because of the configurations is not presented in the NVRAM

Part 2:

Step 2:

* to enable password checking on the console

Step 7:

* $1$mERr$ILwq/b7kc.7X/ejA4Aosn0
* because it is automatically encrypted for security reasons.

Step 8:

* We manually encrypted all the plain text passwords

Part 3:

Step 1:

* When we log in to the Switch
* To provide important iformation

Part 4:

Step 1:

* wr mem or write memory
* as show run command
* Yes, all changes are ecorded

Part 5: